{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["祥符实验室科研设备"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"祥符实验室科研设备","index":0,"n_rows":76,"n_cols":8,"rows_kept":76,"cut":false,"hidden":false,"merged":[[0,0,0,7],[75,0,75,7],[2,0,10,0],[11,0,14,0],[15,0,21,0],[22,0,24,0],[25,0,27,0],[28,0,30,0],[31,0,39,0],[40,0,41,0],[43,0,45,0],[48,0,49,0],[51,0,53,0],[54,0,59,0],[61,0,62,0],[63,0,68,0],[69,0,74,0],[2,1,10,1],[11,1,14,1],[15,1,21,1],[22,1,24,1],[25,1,27,1],[28,1,30,1],[31,1,39,1],[40,1,41,1],[43,1,45,1],[48,1,49,1],[51,1,53,1],[54,1,59,1],[61,1,62,1],[63,1,68,1],[64,3,67,3],[2,7,10,7],[11,7,14,7],[15,7,21,7],[22,7,24,7],[25,7,27,7],[28,7,30,7],[31,7,39,7],[44,7,45,7],[51,7,53,7],[54,7,57,7],[69,7,74,7]]}
["                  祥符实验室科研设备"]
["仪器名称","设备参数/检测能力","序号","检测项目","计费单位","标准费用","检测周期","备注"]
["透射电镜","参数：\n加速电压：80~200kV；\n点分辨率：0.23nm；线分辨率：0.14nm；STEM分辨率：1.0nm；TEM倍率：30~1,500,000；STEM倍率：100~2,000,000。\n检测能力：\n高分子、金属、半导体等材料科学领域以及细胞、组织等生命科学领域的微观形貌成像、元素分析和物相分析\n",1,"普通形貌","元/样品",400,"5个工作日","1、每个样品限0.5h，超时按800元/小时\n2、制样收费：普通碳膜20元/个，其他30元/个)\n3、自主操作培训：500元/h"]
[null,null,2,"形貌高分辨","元/样品",500,"5个工作日"]
[null,null,3,"弱磁另加","元/样品",100,"5个工作日"]
[null,null,4,"能谱-点","元/3点","100(超出30元/点)","5个工作日"]
[null,null,5,"能谱-线","元/次",150,"5个工作日"]
[null,null,6,"能谱-面","元/次",200,"5个工作日"]
[null,null,7,"云视频(非磁)/现场","元/小时",800,"5个工作日"]
[null,null,8,"云视频(弱磁)/现场","元/小时",900,"5个工作日"]
[null,null,9,"自主上机","元/小时",800,"/"]
["X射线显微镜\nXradia 515 Versa（XRM）","参数：\n500nm真实空间分辨率，40nm最小体素；独特的大工作距离下高分辨率；可实现不同类型、尺寸样品高分辨成像；吸收、增强相位成像模式\n检测能力：\n利用X射线无损的本质进行3D成像，对材料孔隙或裂纹、硬组织和软组织以及生物的微观结构、芯片的内部特征或封装可靠性等多种领域样品进行多尺度成像、表征和建模",10,"普通成像(超时加1000/h)","元/样品",1400,"5个工作日","耗材另计，（限1h，超时加1000元/h）数据处理按难度500-1000元/h，特殊扫描另加费，不对外自主上机及培训"]
[null,null,11,"特殊成像附加费用：垂直拼接","元/次",600,"5个工作日"]
[null,null,12,"宽视场附加费用","元/次",600,"5个工作日"]
[null,null,13,"内部定位附加费用","元/次",600,"5个工作日"]
["场发射扫描电镜ZEISS GeminiSEM 360（SEM）","参数：\n二次电子分辨率：1.2nm@1kV,0.7nm@15kV（镜筒内减速）；放大倍率：12~2,000,000倍；加速电压：20V~30kV；无交叉光路设计；镜筒内正光轴上环形二次电子探测器。\n检测能力：\n材料、生物样品的微观形貌成像、元素分析",14,"形貌(弱磁另加100/样)","元/样品",350,"5个工作日","1、每个样品限0.5h，超时按700元/小时,\n2、制样收费：制样时间计入机时,\n3、喷金100元/分钟，\n4、自主操作培训：500元/h"]
[null,null,15,"能谱点","元/3点","100(超出30元/点)","5个工作日"]
[null,null,16,"能谱线","元/次",150,"5个工作日"]
[null,null,17,"能谱面","元/次",200,"5个工作日"]
[null,null,18,"云视频(非磁)/现场","元/小时",700,"5个工作日"]
[null,null,19,"云视频(弱磁)/现场","元/小时",800,"5个工作日"]
[null,null,20,"自主上机","元/小时",700,"/"]
["原子力显微镜Multimode 8（AFM）","参数：\n扫描范围：125um*125um*5um；噪声水平：<0.3ÅRMS；\n纵向分辨率：0.1nm，横向分辨率：1nm\n检测能力：\n气/液相微区成像，力学、磁学、电学性能表征",21,"形貌/粗糙度/厚度","元/样品",400,"5个工作日","耗材另计：探针因样品问题损坏需另计费用，（每个样限时1h,超时按形貌/粗糙度/厚度400元/小时，液下模式1000元/小时，其他模式600元/小时），自主操作培训：300元/h"]
[null,null,22,"液下模式","元/样品",1000,"5个工作日"]
[null,null,23,"其他模式600元起","元/样品",600,"5个工作日"]
["激光共聚焦显微镜LSM 900","参数：\n放大倍率：100~630x；横向分辨率：120nm；Z轴驱动器：最小步进10nm；扫描分辨率：32*1-6144*6144像素；扫描速度：8幅/秒（1024*256）；2幅/秒（1024*1024）；扫描控制：0.5-40倍连续可调，360°自由旋转，精度0.1°\n检测能力：\n细胞形态定位、立体结构重组、动态变化过程等研究，并提供定量荧光测定、定量图像分析等",24,"共聚焦","元/样品",400,"5个工作日","1、每个样限时1h，超时按400元/小时\n2、自主操作培训：300元/h"]
[null,null,25,"Airyscan超分辨","元/样品",600,"5个工作日"]
[null,null,26,"自主上机","元/小时",400,"/"]
["基质辅助激光解吸电离飞行质量质谱（MALDI-TOFMS）","质量范围：>500,000Da；分辨率线性模式≥1,100(cytochromeC,m/z12361)，反射模式>26,000(多肽)；串联质谱（TOF/TOF）稳定性：外较准能保持24小时（多肽混合物）\n检测能力：\n1.适用于各类大分子化合物的分析，包括蛋白质/多肽、核酸、多糖、合成聚合物等和磷脂类化合物的测定。\n2.可升级适用于高通量的蛋白质组学研究，包括蛋白质肽质量指纹谱测定，多肽序列分析蛋白质翻译后修饰鉴定，蛋白质相互作用和\n自上而下蛋白质序列分析等研究",27,"小分子化合物质量小于2000","元/样品",200,"5个工作日","标准品消耗部分用户自费，自主操作：800元/h\n同一批次，使用相同方法时：\n1~100样，50元/样\n101样以上,25元/样"]
[null,null,28,"高分子聚合物、多糖、蛋白、核酸、有机金属等","元/样品",300,"5个工作日"]
[null,null,29,"方法建立费","元/样品",400,"5个工作日"]
["电感耦合等离子体质谱(ICPMS)","参数：\n质谱范围：1-280amu。\n离子源：频率为34MHz，功率范围400-1600W，连续1w可调\n四级杆驱动频率≥2.5MHz\n数据采集速度：>100,000个临时数据点/秒\n采样锥口径为1.1mm，截取锥口径为0.9mm，超级截取锥口径为1.0mm\n检测能力：\n1.电感耦合等离子体质谱仪要求能适用于应用领域广泛的各种样品的元素分析、同位素分析分析任务满足环境、食品、医药、地质、金属材料、生物样品、化工材料分析等等。\n2.能进行样品定性、半定量、定量、同位素比分析。",30,"前处理：",null,"case","5个工作日","计费方式二选一：由测试老师根据收费标准，于实际测试后核定，120元起/样，不支持自主上机测试"]
[null,null,31,"1级：简单稀释、过滤（40/样品）","元/样品",40,"5个工作日"]
[null,null,32,"一般消解（混酸、加热）120/样","元/样品",200,"5个工作日"]
[null,null,33,"全扫半定量","元/样品",300,"5个工作日"]
[null,null,34,"常规定量标准曲线（标曲+元素）200元/次（1个元素），每增加1个元素加收40元","元/样品",200,"5个工作日"]
[null,null,35,"常规定量，120/样","元/样品",120,"5个工作日"]
[null,null,36,"标加法费用=（基本费用+元素费用）*样品个数，400/样","元/样品",400,"5个工作日"]
[null,null,37,"高纯或者痕量分析费用-系统清洗3小时，2000/样","元/样品",2000,"5个工作日"]
[null,null,38,"技术服务费用：首次委托条件优选，费用范围从0-2000，由测试老师优选测试条件后选定2000/次",null,2000,"5个工作日"]
["分选型流式细胞仪","三根非共线可独立激发激光器：488nm(16mW)、405nm(36mW)、561nm(40mW)，同时激发8色荧光，激光功率＜50mw；PMT检测器(非FAPD类)，灵敏度：FITC＜53MESF、PE＜9MESF\n具备自动液滴断点监控和堵塞监测系统，液滴分析精度高达1/32；分析速度：≥40000细胞/秒，分选速度：≥34000细胞/秒；分选纯度：＞98%；回收率：＞80%",39,"细胞分选-送样","元/样品",200,"5个工作日","耗材自备或按实结算"]
[null,null,40,"细胞分选-连续操作","元/小时",500,"5个工作日"]
["DNA合成仪","参数：合成仪的通量：28柱；在线脱保护监测：28个独立的Trityl在线监测器，实时监测耦合效率；合成产物种类：DNA/RNA/LNA荧光标记/探针、甲基化、硫代及其他特殊基团修饰等；\n合成周期：(20bp)1小时;每个循环时间：3-4分钟;耦合效率：>99.5%;合成产物的长度：200bp; 最大合成规模：40μmol；成产物承载方式：合成柱；碱基瓶位：12个；试剂瓶位：9个；碱基驱动方式：微型液体电磁阀；试剂驱动方式：微型气体电磁阀；试剂通用。",41,"DNA合成","元/小时",120,"5个工作日","耗材自备或按实结算"]
["旋转流变仪（室温~200℃）","参数：最小振荡扭矩(nN.m)：5 ; 最小稳态剪切扭矩(nN.m)：5 ; 最大扭矩(mN.m)：200 ;扭矩分辨率(nN.m)：0.1;最小频率(Hz)：10-7;最大频率(Hz)：100Hz;最小角速率(rad/s)：0;最大角速率(rad/s)：300\n测试能力：\n适用于多种不同模量的样品类型，尤其适用于中低模量、易挥发的水凝胶类样品测试。通过测量剪切速率、剪切应力、振荡频率、应力应变振幅等流变数据，计算样品的黏度、储能模量、损耗模量、Tanδ等流变学参数。测试模式包含受控应力模式（稳态、瞬态、振荡）和受控应变模式（稳态、瞬态、迭代振荡）。",42,"室温","元/样品",100,"5个工作日","单个样品限时15min，超时按400元/h收费。"]
[null,null,43,"变温","元/小时",400,"5个工作日","/"]
[null,null,44,"自主上机","元/小时",200,"/"]
["液相色谱仪","流量范围：可设定0.001-10mL/min；流量精度：<0.07%RSD，或<0.02minSD，以较大者为准；组成范围：可设置:0-100%；信号数量：单波长和双波长检测；",45,null,"元/小时",140,"5个工作日","耗材自备或按实结算"]
["多功能成像系统","凝胶成像分辨率高，成像面积大，可满足科研需求;光源强度高、灵敏度高、均一性好，用于SYBRGold, SYBRGreen, SYBRSafe, SYPROOrange, SYPRORubyUltraPower, Ethidiumbromide, GelGreen,GelRed等染料的检测;可升级三色侧照光源，用于Cy2、Cy3和Cy5染色的2D胶成像;可观察3D图像及输出;对于多色荧光图像，可以切换通道，单独分析某个通道或多通道的图像",47,null,"元/小时",100,"5个工作日","耗材自备或按实结算"]
["紫外分光光度计","选配积分球：分析波长范围可扩大至1400nm近红外区域\n高性能光路系统：搭配岛津自有的高性能Lo-Ray-Light光栅，实现低杂散光<0.005%T",48,null,"元/小时",200,"5个工作日","耗材自备或按实结算"]
[null,null,49,"自主上机","元/小时",160,"/","/"]
["荧光定量PCR系统","大于六个检测通道，可同时实现≥5重PCR，可同时检测≥5个靶基因；\n具有FRET检测通道；",50,null,"元/时",250,"5个工作日","耗材自备或按实结算"]
["纳米粒度电位仪","测量范围(最大粒径)：0.3nm-10μm*(Pro)；0.3nm-10μm*(15μmΓ)(Lab/Ultra)\n最小样品容积：12μL(Pro)；3μL(Lab/Ultra)\n最小浓度-非侵入式背散射(NIBS)(173度)：0.1mg/mL15kDa蛋白质(Pro/Ultra)；\n最小浓度-前向散射(13度)：10mg/mL15kDa蛋白质(Lab/Pro/UltraBlue)；5mg/mL15kDa蛋白质(Lab/Pro/UltraRed)\n最小浓度-侧向散射(90度)：1mg/mL15kDa蛋白质(Lab/UltraBlue)；0.3mg/mL15kDa蛋白质(Lab/UltraRed)\n最小浓度-多角动态光散射(MADLS)：1mg/mL15kDa蛋白质(UltraBlue和Red)",51,"自主上机","元/小时",400,null,"送样检测按样品算，自主上机按时间算，耗材自费"]
[null,null,52,"Zeta电位","元/样品",120,"5个工作日"]
[null,null,53,"粒径","元/样品",120,"5个工作日"]
["荧光光谱仪","紫外可见检测器光谱范围为200-870nm;近红外检测器光谱范围为300-1700nm;\n使用450W除臭氧氙灯(集成式电源)，可以显示功率、电压、电流和使用时间；\n标准信噪比：20000：1，睡拉曼峰测试，激发波长350nm，狭缝5nm，积分时间1s;\n使用375nm皮秒脉冲二极管激光器,典型脉冲宽度为55ps，重复频率为20kHz-20MHz。\n检测能力：稳态光谱、荧光寿命、绝对量子产率、时间分辨光谱",54,"激发/发射光谱（紫外-可见区）","元/样品",160,"5个工作日","耗材自备或按实结算"]
[null,null,55,"激发/发射光谱（红外区）","元/样品",200,"5个工作日"]
[null,null,56,"荧光寿命/量子产率/上转换测试/（紫外-可见区）","元/样品",300,"5个工作日"]
[null,null,57,"荧光寿命/量子产率/上转换测试/（红外区）","元/样品",400,"5个工作日"]
[null,null,58,"变温测试（77K-500K）","元/样品",600,"5个工作日","限1小时，超时加收600元/小时"]
[null,null,59,"自主上机","元/小时",400,"/"]
["全自动单丝测试仪\n(品牌：TEXTECHNO，型号：FAVIMAT + AIROBOT Ⅱ)","样品要求：适用于名义长度不小于20mm的化学纤维短纤维，50根以上足量，线密度已知",60,"短纤维拉伸性能","元/样品",600,"5个工作日","/"]
["电子织物强力仪\n（品牌：莱州电子，型号：YG065H）","量程：单纱强力100.0N，织物强力2000N；拉伸速度：2mm/min-1200mm/min;返回速度：2mm/min-1000mm/min；最大设定拉伸次数：99次；隔距：25-500mm",61,"织物拉伸性能（断裂强力/伸长率）","元/样品",600,"5个工作日","/"]
[null,null,62,"单纱拉伸性能（断裂强力/伸长率）","元/样品",600]
["高性能计算服务器",null,63,"高性能计算CPU8台*56核","元/核/时",0.2,"5个工作日"]
[null,null,67,null,"元/卡时",6,"5个工作日","低谷 00:00-18:00"]
[null,null,68,null,"元/卡时",8,"5个工作日","平峰 08:00-18:00"]
[null,null,69,null,"元/卡时",10,"5个工作日","高峰 18:00-24:00"]
[null,null,72,null,"万元/8卡包月",4,"5个工作日"]
[null,null,73,"存储","元/TB/年",400,"5个工作日"]
["生物医学计算服务","快速分析标准模块:基因组(生殖系、体细胞变异)+转录组(NGS差异表达、单细胞)+表观遗传(甲基化WGBS、甲基化芯片)+GWAS分析",74,"快速分析标准模块","元/次",50,"5个工作日","CPU&GPU：5折（自主安装环境），\n2.5折（开发一键式分析平台集成工具）"]
[null,"快速分析专业模块:基因组(生殖系、体细胞变异)+转录组(NGS差表达、单细胞)+表观遗传(甲基化WGBS、甲基化芯片)+GWAS分析+腕表数据预处理+酵母荧光显微计数",75,"快速分析专业模块","元/次",80,"5个工作日"]
[null,"快速分析高级推理模块:基因组(生殖系、体细胞变异)+转录组(NGS差异表达、单细胞)+表观遗传(甲基化WGBS、甲基化芯片)+GWAS分析+腕表数据预处理+酵母荧光显微计数+遗传疾病辅助诊断+肿瘤用药辅助指导",76,"快速分析高级推理模块","元/次",150,"5个工作日"]
[null,"自定义计算模块-智能推理模块",77,"自定义计算模块-智能推理模块","元/项","30000元/项(面议、合同)","5个工作日"]
[null,"自定义计算模块-多模态影像分析",78,"自定义计算模块-多模态影像分析","元/项","15000元/项(面议、合同)","5个工作日"]
[null,"自定义计算模块-多组学分析",79,"自定义计算模块-多组学分析","元/项","8000元/项(面议、合同)","5个工作日"]
["按时间收费设备测试时长<10min按15min计，10min≤测试时长<40min按0.5h计，40min≤测试时长<1h按1h计；\n加急加收50%费用。"]